* Sea-Bird SBE 9 Data File:
* FileName = C:\data\TN443\raw\08301.hdr
* Software Version Seasave V 7.26.7.107
* Temperature SN = 2309
* Conductivity SN = 2319
* Number of Bytes Per Scan = 41
* Number of Voltage Words = 4
* Number of Scans Averaged by the Deck Unit = 1
* Append System Time to Every Scan
* System UpLoad Time = Apr 19 2025 23:07:29
* NMEA Latitude = 14 04.45 N
* NMEA Longitude = 089 18.35 E
* NMEA UTC (Time) = Apr 19 2025  23:07:40
* Store Lat/Lon Data = Append to Every Scan
* SBE 11plus V 5.2
* number of scans to average = 1
* pressure baud rate = 9600
* NMEA baud rate = 4800
* GPIB address = 1
* advance primary conductivity  0.073 seconds
* advance secondary conductivity  0.073 seconds
* autorun on power up is disabled
* S>
** Cruise: TN443
** Cast: 08301
** Location: 
** Date: 2025-04-19
** Water Depth: 
** Operator: GC
* System UTC = Apr 19 2025 23:07:29
*END*
