* Sea-Bird SBE 9 Data File:
* FileName = C:\SBE_DATA\185_OISO19\La18_0028_O3_D.DAT
* Software Version Seasave Win32 V 5.35a
* Temperature SN = 1821
* Conductivity SN = 2317
* Number of Bytes Per Scan = 37
* Number of Voltage Words = 5
* Number of Scans Averaged by the Deck Unit = 1
* Append System Time to Every Scan
* System UpLoad Time = Jan 18 2011 00:35:15
** Ship:       
** Cruise:     
** Station:   O3 D 
** Latitude:  35 00.00 S
** Longitude: 053 29.98 E 
# nquan = 22
# nvalues = 1007                        
# units = specified
# name 0 = nbf: Bottles Fired
# name 1 = prDM: Pressure, Digiquartz [db]
# name 2 = depSM: Depth [salt water, m]
# name 3 = t090C: Temperature [ITS-90, deg C]
# name 4 = c0S/m: Conductivity [S/m]
# name 5 = sal00: Salinity [PSU]
# name 6 = potemp090C: Potential Temperature [ITS-90, deg C]
# name 7 = sigma-é00: Density [sigma-theta, Kg/m^3]
# name 8 = v0: Voltage 0
# name 9 = sbeox0Mm/Kg: Oxygen, SBE 43 [umol/Kg]
# name 10 = v2: Voltage 2
# name 11 = flECO-AFL: Fluorescence, Wetlab ECO-AFL/FL [mg/m^3]
# name 12 = flECO-AFL: Fluorescence, Wetlab ECO-AFL/FL [mg/m^3]
# name 13 = dz/dtM: Descent Rate [m/s]
# name 14 = scan: Scan Count
# name 15 = depSM: Depth [salt water, m], lat = 40
# name 16 = sal00: Salinity [PSU]
# name 17 = potemp090C: Potential Temperature [ITS-90, deg C]
# name 18 = sigma-é00: Density [sigma-theta, Kg/m^3]
# name 19 = dz/dtM: Descent Rate [m/s], WS = 2
# name 20 = nbin: number of scans per bin
# name 21 = flag: flag
# span 0 =          0,          0       
# span 1 =      5.000,   1010.000       
# span 2 =      4.947,    999.831       
# span 3 =     7.3316,    20.2279       
# span 4 =   3.560249,   4.861486       
# span 5 =    34.5278,    35.5138       
# span 6 =     7.2297,    20.2275       
# span 7 =    24.9892,    27.0147       
# span 8 =     1.7263,     2.6208       
# span 9 =    200.398,    243.949       
# span 10 =     0.0354,     0.1569      
# span 11 =    -0.0849,     1.4807      
# span 12 =    -0.0849,     1.4807      
# span 13 =     -1.069,      1.767      
# span 14 =        -72,      41653      
# span 15 =      4.962,    999.830      
# span 16 =    34.5278,    35.5138      
# span 17 =     7.2297,    20.2270      
# span 18 =    24.9894,    27.0147      
# span 19 =     -0.076,      1.765      
# span 20 =          1,        139      
# span 21 = 0.0000e+00, 0.0000e+00      
# interval = decibars: 1                
# start_time = Jan 18 2011 00:35:15
# bad_flag = -9.990e-29
# sensor 0 = Frequency  0  temperature, 1821, 2010/11/19
# sensor 1 = Frequency  1  conductivity, 2317, 2010/11/19, cpcor = -9.5700e-08
# sensor 2 = Frequency  2  pressure, 02/05/2005
# sensor 3 = Extrnl Volt  0  Oxygen, SBE, primary, 0563, 2010/12/21
# sensor 4 = Extrnl Volt  2  WET Labs, ECO_AFL
# sensor 5 = Extrnl Volt  9  surface irradiance (SPAR), degrees = 0.0
# datcnv_date = Jan 29 2011 21:06:08, 7.18
# datcnv_in = C:\SeaBirdDataProcessing\185_OISO19\st3\la18_0028_03d.dat C:\SeaBirdDataProcessing\185_OISO19\precalib2010.CON
# datcnv_skipover = 0
# wildedit_date = Jan 29 2011 21:07:06, 7.18
# wildedit_in = C:\SeaBirdDataProcessing\185_OISO19\st3\la18_0028_03d.cnv
# wildedit_pass1_nstd = 2.0
# wildedit_pass2_nstd = 20.0
# wildedit_pass2_mindelta = 0.000e+000
# wildedit_npoint = 100
# wildedit_vars = prDM depSM t090C c0S/m sal00 potemp090C sigma-é00 v0 sbeox0Mm/Kg v2 flECO-AFL flECO-AFL dz/dtM
# wildedit_excl_bad_scans = yes
# filter_date = Jan 29 2011 21:07:39, 7.18
# filter_in = C:\SeaBirdDataProcessing\185_OISO19\st3\la18_0028_03d.cnv
# filter_low_pass_tc_A = 0.030
# filter_low_pass_tc_B = 0.150
# filter_low_pass_A_vars = depSM sal00 potemp090C sigma-é00 v0 sbeox0Mm/Kg v2 flECO-AFL flECO-AFL dz/dtM
# filter_low_pass_B_vars = prDM
# loopedit_date = Jan 29 2011 21:09:29, 7.18
# loopedit_in = C:\SeaBirdDataProcessing\185_OISO19\st3\la18_0028_03d.cnv
# loopedit_percentMeanSpeed: minV = 0.250, ws = 300, percent = 20.00                                                      
# loopedit_surfaceSoak: do not remove                                                                                     
# loopedit_excl_bad_scans = yes
# Derive_date = Jan 29 2011 21:10:12, 7.18
# Derive_in = C:\SeaBirdDataProcessing\185_OISO19\st3\la18_0028_03d.cnv C:\SeaBirdDataProcessing\185_OISO19\precalib2010.CON
# derive_time_window_dzdt = seconds: 2
# binavg_date = Jan 29 2011 21:11:05, 7.18
# binavg_in = C:\SeaBirdDataProcessing\185_OISO19\st3\la18_0028_03d.cnv
# binavg_bintype = decibars
# binavg_binsize = 1
# binavg_excl_bad_scans = yes
# binavg_skipover = 0
# binavg_surface_bin = no, min = 0.000, max = 0.000, value = 0.000
# file_type = ascii
*END*
