* Sea-Bird SBE 9 Data File:
* FileName = C:\SBE_DATA\185_OISO19\Lb18_1500_Oiso21_D.HDR
* Software Version Seasave Win32 V 5.35a
* Temperature SN = 1821
* Conductivity SN = 2317
* Number of Bytes Per Scan = 37
* Number of Voltage Words = 5
* Number of Scans Averaged by the Deck Unit = 1
* Append System Time to Every Scan
* System UpLoad Time = Feb 18 2011 15:01:04
** Ship:       MD FNIN
** Cruise:     185
** Station:    21 D
** Latitude:   25 59.99 S
** Longitude:  057 29.99 E
** Descente
# nquan = 21
# nvalues = 130233                      
# units = specified
# name 0 = nbf: Bottles Fired
# name 1 = prDM: Pressure, Digiquartz [db]
# name 2 = depSM: Depth [salt water, m], lat = -40.00
# name 3 = t090C: Temperature [ITS-90, deg C]
# name 4 = c0S/m: Conductivity [S/m]
# name 5 = sal00: Salinity, Practical [PSU]
# name 6 = potemp090C: Potential Temperature [ITS-90, deg C]
# name 7 = sigma-é00: Density [sigma-theta, Kg/m^3]
# name 8 = v0: Voltage 0
# name 9 = sbeox0Mm/Kg: Oxygen, SBE 43 [umol/Kg]
# name 10 = v2: Voltage 2
# name 11 = flECO-AFL: Fluorescence, WET Labs ECO-AFL/FL [mg/m^3]
# name 12 = flECO-AFL: Fluorescence, WET Labs ECO-AFL/FL [mg/m^3]
# name 13 = dz/dtM: Descent Rate [m/s]
# name 14 = scan: Scan Count
# name 15 = depSM: Depth [salt water, m], lat = 40
# name 16 = sal00: Salinity, Practical [PSU]
# name 17 = potemp090C: Potential Temperature [ITS-90, deg C]
# name 18 = sigma-é00: Density [sigma-theta, Kg/m^3]
# name 19 = dz/dtM: Descent Rate [m/s], WS = 2
# name 20 = flag: flag
# span 0 =          0,          0       
# span 1 =      9.662,   5110.914       
# span 2 =      9.573,   5011.911       
# span 3 =   -98.9762,    99.0000       
# span 4 =   3.144407,   5.464410       
# span 5 =   -49.7654,   236.9949       
# span 6 =   -92.2020,    94.4374       
# span 7 =  -156.5288,  1495.4807       
# span 8 =     1.0761,     2.7319       
# span 9 =      2.534, 3.9275e+07       
# span 10 =     0.0784,     0.5979      
# span 11 =    -0.0875,     3.2604      
# span 12 =    -0.0875,     3.2604      
# span 13 =     -0.836,      1.787      
# span 14 =          1,     130233      
# span 15 =      9.588,   5011.884      
# span 16 = -1999.0000,  1999.0000      
# span 17 =  -102.0009,    95.2758      
# span 18 =  -157.5277,  1999.0000      
# span 19 =     -0.829,      1.766      
# span 20 = 0.0000e+00, 0.0000e+00      
# interval = seconds: 0.0416667
# start_time = Feb 18 2011 15:01:05 [System UTC, first data scan.]
# bad_flag = -9.990e-29
# <Sensors count="15" >
#   <sensor Channel="1" >
#     <!-- Frequency 0, Temperature -->
#     <TemperatureSensor SensorID="55" >
#       <SerialNumber>1821</SerialNumber>
#       <CalibrationDate>2010/11/10</CalibrationDate>
#       <UseG_J>1</UseG_J>
#       <A>0.00000000e+000</A>
#       <B>0.00000000e+000</B>
#       <C>0.00000000e+000</C>
#       <D>0.00000000e+000</D>
#       <F0_Old>0.000</F0_Old>
#       <G>4.87571262e-003</G>
#       <H>6.89355063e-004</H>
#       <I>3.03221299e-005</I>
#       <J>2.60451786e-006</J>
#       <F0>1000.000</F0>
#       <Slope>1.00000000</Slope>
#       <Offset>0.0000</Offset>
#     </TemperatureSensor>
#   </sensor>
#   <sensor Channel="2" >
#     <!-- Frequency 1, Conductivity -->
#     <ConductivitySensor SensorID="3" >
#       <SerialNumber>2317</SerialNumber>
#       <CalibrationDate>2010/11/10</CalibrationDate>
#       <UseG_J>1</UseG_J>
#       <!-- Cell const and series R are applicable only for wide range sensors. -->
#       <SeriesR>0.0000</SeriesR>
#       <CellConst>2000.0000</CellConst>
#       <ConductivityType>0</ConductivityType>
#       <Coefficients equation="0" >
#         <A>0.00000000e+000</A>
#         <B>0.00000000e+000</B>
#         <C>0.00000000e+000</C>
#         <D>0.00000000e+000</D>
#         <M>0.0</M>
#         <CPcor>-9.57000000e-008</CPcor>
#       </Coefficients>
#       <Coefficients equation="1" >
#         <G>-1.07859966e+001</G>
#         <H>1.47329303e+000</H>
#         <I>-1.75348756e-004</I>
#         <J>7.37392413e-005</J>
#         <CPcor>-9.57000000e-008</CPcor>
#         <CTcor>3.2500e-006</CTcor>
#         <!-- WBOTC not applicable unless ConductivityType = 1. -->
#         <WBOTC>0.00000000e+000</WBOTC>
#       </Coefficients>
#       <Slope>1.00000000</Slope>
#       <Offset>0.00000</Offset>
#     </ConductivitySensor>
#   </sensor>
#   <sensor Channel="3" >
#     <!-- Frequency 2, Pressure, Digiquartz with TC -->
#     <PressureSensor SensorID="45" >
#       <SerialNumber>0402</SerialNumber>
#       <CalibrationDate>02/05/2005</CalibrationDate>
#       <C1>-4.471217e+004</C1>
#       <C2>7.207370e-002</C2>
#       <C3>1.279440e-002</C3>
#       <D1>3.850500e-002</D1>
#       <D2>0.000000e+000</D2>
#       <T1>2.993439e+001</T1>
#       <T2>-2.595180e-004</T2>
#       <T3>3.740980e-006</T3>
#       <T4>3.368070e-009</T4>
#       <Slope>0.99995000</Slope>
#       <Offset>-0.39210</Offset>
#       <T5>0.000000e+000</T5>
#       <AD590M>1.118000e-002</AD590M>
#       <AD590B>-8.461320e+000</AD590B>
#     </PressureSensor>
#   </sensor>
#   <sensor Channel="4" >
#     <!-- Frequency 3, Temperature, 2 -->
#     <TemperatureSensor SensorID="55" >
#       <SerialNumber>2537</SerialNumber>
#       <CalibrationDate>10-Nov-2005</CalibrationDate>
#       <UseG_J>1</UseG_J>
#       <A>0.00000000e+000</A>
#       <B>0.00000000e+000</B>
#       <C>0.00000000e+000</C>
#       <D>0.00000000e+000</D>
#       <F0_Old>0.000</F0_Old>
#       <G>4.36971789e-003</G>
#       <H>6.46020675e-004</H>
#       <I>2.29913091e-005</I>
#       <J>2.09788553e-006</J>
#       <F0>1000.000</F0>
#       <Slope>1.00000000</Slope>
#       <Offset>0.0000</Offset>
#     </TemperatureSensor>
#   </sensor>
#   <sensor Channel="5" >
#     <!-- Frequency 4, Conductivity, 2 -->
#     <ConductivitySensor SensorID="3" >
#       <SerialNumber>2215</SerialNumber>
#       <CalibrationDate>30-Sep-2005</CalibrationDate>
#       <UseG_J>1</UseG_J>
#       <!-- Cell const and series R are applicable only for wide range sensors. -->
#       <SeriesR>0.0000</SeriesR>
#       <CellConst>2000.0000</CellConst>
#       <ConductivityType>0</ConductivityType>
#       <Coefficients equation="0" >
#         <A>0.00000000e+000</A>
#         <B>0.00000000e+000</B>
#         <C>0.00000000e+000</C>
#         <D>0.00000000e+000</D>
#         <M>0.0</M>
#         <CPcor>-9.57000000e-008</CPcor>
#       </Coefficients>
#       <Coefficients equation="1" >
#         <G>-1.04011406e+001</G>
#         <H>1.53628070e+000</H>
#         <I>-2.93388335e-003</I>
#         <J>3.08600206e-004</J>
#         <CPcor>-9.57000000e-008</CPcor>
#         <CTcor>3.2500e-006</CTcor>
#         <!-- WBOTC not applicable unless ConductivityType = 1. -->
#         <WBOTC>0.00000000e+000</WBOTC>
#       </Coefficients>
#       <Slope>1.00000000</Slope>
#       <Offset>0.00000</Offset>
#     </ConductivitySensor>
#   </sensor>
#   <sensor Channel="6" >
#     <!-- A/D voltage 0, Oxygen, SBE 43 -->
#     <OxygenSensor SensorID="38" >
#       <SerialNumber>0563</SerialNumber>
#       <CalibrationDate>21-Dec-2010</CalibrationDate>
#       <Use2007Equation>0</Use2007Equation>
#       <CalibrationCoefficients equation="0" >
#         <!-- Coefficients for Owens-Millard equation. -->
#         <Boc>0.0000</Boc>
#         <Soc>4.9690e-001</Soc>
#         <offset>-0.4999</offset>
#         <Pcor>1.50e-004</Pcor>
#         <Tcor>-0.0330</Tcor>
#         <Tau>1.3</Tau>
#       </CalibrationCoefficients>
#       <CalibrationCoefficients equation="1" >
#         <!-- Coefficients for Sea-Bird equation - SBE calibration in 2007 and later. -->
#         <Soc>0.0000e+000</Soc>
#         <offset> 0.0000</offset>
#         <A> 0.0000e+000</A>
#         <B> 0.0000e+000</B>
#         <C> 0.0000e+000</C>
#         <D0> 2.5826e+000</D0>
#         <D1> 1.92634e-004</D1>
#         <D2>-4.64803e-002</D2>
#         <E> 0.0000e+000</E>
#         <Tau20> 0.0000</Tau20>
#         <H1>-3.3000e-002</H1>
#         <H2> 5.0000e+003</H2>
#         <H3> 1.4500e+003</H3>
#       </CalibrationCoefficients>
#     </OxygenSensor>
#   </sensor>
#   <sensor Channel="7" >
#     <!-- A/D voltage 1, Free -->
#   </sensor>
#   <sensor Channel="8" >
#     <!-- A/D voltage 2, Fluorometer, WET Labs ECO-AFL/FL -->
#     <FluoroWetlabECO_AFL_FL_Sensor SensorID="20" >
#       <SerialNumber>FLRTD-102</SerialNumber>
#       <CalibrationDate>15-Dec-2003</CalibrationDate>
#       <ScaleFactor>6.44400000e+000</ScaleFactor>
#       <!-- Dark output -->
#       <Vblank>0.0920</Vblank>
#     </FluoroWetlabECO_AFL_FL_Sensor>
#   </sensor>
#   <sensor Channel="9" >
#     <!-- A/D voltage 3, Free -->
#   </sensor>
#   <sensor Channel="10" >
#     <!-- A/D voltage 4, Free -->
#   </sensor>
#   <sensor Channel="11" >
#     <!-- A/D voltage 5, Free -->
#   </sensor>
#   <sensor Channel="12" >
#     <!-- A/D voltage 6, Free -->
#   </sensor>
#   <sensor Channel="13" >
#     <!-- A/D voltage 7, Free -->
#   </sensor>
#   <sensor Channel="14" >
#     <!-- SPAR voltage, Unavailable -->
#   </sensor>
#   <sensor Channel="15" >
#     <!-- SPAR voltage, SPAR/Surface Irradiance -->
#     <SPAR_Sensor SensorID="51" >
#       <SerialNumber></SerialNumber>
#       <CalibrationDate></CalibrationDate>
#       <ConversionFactor>0.00000000</ConversionFactor>
#       <RatioMultiplier>0.00000000</RatioMultiplier>
#     </SPAR_Sensor>
#   </sensor>
# </Sensors>
# datcnv_date = May 23 2013 20:42:45, 7.21k [datcnv_vars = 15]
# datcnv_in = C:\SBE_DATA\OISO19\185_OISO19_ALLsave\lb18_1500_oiso21_d.dat C:\SBE_DATA\OISO19\185_OISO19_ALLsave\lb18_1500_oiso21_d.CON
# datcnv_skipover = 0
# datcnv_ox_hysteresis_correction = no
# datcnv_ox_tau_correction = yes
# wildedit_date = May 23 2013 20:43:40, 7.21k
# wildedit_in = C:\SBE_DATA\OISO19\185_OISO19_ALLsave\lb18_1500_oiso21_d.cnv
# wildedit_pass1_nstd = 2.0
# wildedit_pass2_nstd = 20.0
# wildedit_pass2_mindelta = 0.000e+000
# wildedit_npoint = 100
# wildedit_vars = prDM depSM t090C c0S/m sal00 potemp090C sigma-é00 v0 sbeox0Mm/Kg v2 flECO-AFL flECO-AFL dz/dtM
# wildedit_excl_bad_scans = yes
# filter_date = May 23 2013 20:44:15, 7.21k
# filter_in = C:\SBE_DATA\OISO19\185_OISO19_ALLsave\lb18_1500_oiso21_d.cnv
# filter_low_pass_tc_A = 0.030
# filter_low_pass_tc_B = 0.150
# filter_low_pass_A_vars = depSM sal00 potemp090C sigma-é00 v0 sbeox0Mm/Kg v2 flECO-AFL flECO-AFL dz/dtM
# filter_low_pass_B_vars = prDM
# loopedit_date = May 23 2013 20:45:00, 7.21k
# loopedit_in = C:\SBE_DATA\OISO19\185_OISO19_ALLsave\lb18_1500_oiso21_d.cnv
# loopedit_percentMeanSpeed: minV = 0.250, ws = 300, percent = 20.00                                                      
# loopedit_surfaceSoak: do not remove                                                                                     
# loopedit_excl_bad_scans = yes
# Derive_date = May 23 2013 20:45:41, 7.21k [derive_vars = 5]
# Derive_in = C:\SBE_DATA\OISO19\185_OISO19_ALLsave\lb18_1500_oiso21_d.cnv C:\SBE_DATA\OISO19\185_OISO19_ALLsave\precalib2010_noNMEA_TCPTC.CON
# derive_time_window_dzdt = seconds: 2
# file_type = ascii
*END*
