* Sea-Bird SBE 9 Data File:
* FileName = C:\SBE_DATA\185_OISO19\La26_1900_OISO19_09D.DAT
* Software Version Seasave Win32 V 5.35a
* Temperature SN = 1821
* Conductivity SN = 2317
* Number of Bytes Per Scan = 37
* Number of Voltage Words = 5
* Number of Scans Averaged by the Deck Unit = 1
* Append System Time to Every Scan
* System UpLoad Time = Jan 26 2011 19:01:13
** Ship:       MD FNIN
** Cruise:     185
** Station:    09 D
** Latitude:   48° 29.99 S
** Longitude:  64 59.99 E
# nquan = 22
# nvalues = 999                         
# units = specified
# name 0 = nbf: Bottles Fired
# name 1 = prDM: Pressure, Digiquartz [db]
# name 2 = depSM: Depth [salt water, m]
# name 3 = t090C: Temperature [ITS-90, deg C]
# name 4 = c0S/m: Conductivity [S/m]
# name 5 = sal00: Salinity [PSU]
# name 6 = potemp090C: Potential Temperature [ITS-90, deg C]
# name 7 = sigma-é00: Density [sigma-theta, Kg/m^3]
# name 8 = v0: Voltage 0
# name 9 = sbeox0Mm/Kg: Oxygen, SBE 43 [umol/Kg]
# name 10 = v2: Voltage 2
# name 11 = flECO-AFL: Fluorescence, Wetlab ECO-AFL/FL [mg/m^3]
# name 12 = flECO-AFL: Fluorescence, Wetlab ECO-AFL/FL [mg/m^3]
# name 13 = dz/dtM: Descent Rate [m/s]
# name 14 = scan: Scan Count
# name 15 = depSM: Depth [salt water, m], lat = 40
# name 16 = sal00: Salinity [PSU]
# name 17 = potemp090C: Potential Temperature [ITS-90, deg C]
# name 18 = sigma-é00: Density [sigma-theta, Kg/m^3]
# name 19 = dz/dtM: Descent Rate [m/s], WS = 2
# name 20 = nbin: number of scans per bin
# name 21 = flag: flag
# span 0 =          0,          0       
# span 1 =      7.000,   1003.000       
# span 2 =      6.949,    992.922       
# span 3 =     2.2778,     6.1555       
# span 4 =   3.028220,   3.334052       
# span 5 =    33.6825,    34.6599       
# span 6 =     2.2475,     6.1547       
# span 7 =    26.4921,    27.6790       
# span 8 =     1.4348,     2.6141       
# span 9 =    169.403,    321.378       
# span 10 =     0.0380,     0.3676      
# span 11 =    -0.0518,     4.1974      
# span 12 =    -0.0518,     4.1974      
# span 13 =     -0.491,      1.756      
# span 14 =        666,      25227      
# span 15 =      6.946,    992.917      
# span 16 =    33.6825,    34.6599      
# span 17 =     2.2475,     6.1547      
# span 18 =    26.4921,    27.6790      
# span 19 =     -0.293,      1.752      
# span 20 =         10,         74      
# span 21 = 0.0000e+00, 0.0000e+00      
# interval = decibars: 1                
# start_time = Jan 26 2011 19:01:13
# bad_flag = -9.990e-29
# sensor 0 = Frequency  0  temperature, primary, 1821, 2010/11/10
# sensor 1 = Frequency  1  conductivity, primary, 2317, 2010/11/10, cpcor = -9.5700e-08
# sensor 2 = Frequency  2  pressure, 0402, 02/05/2005
# sensor 3 = Frequency  3  temperature, secondary, 2537, 10-Nov-2005
# sensor 4 = Frequency  4  conductivity, secondary, 2215, 30-Sep-2005, cpcor = -9.5700e-08
# sensor 5 = Extrnl Volt  0  Oxygen, SBE, primary, 0563, 2010/12/21
# sensor 6 = Extrnl Volt  2  WET Labs, ECO_AFL
# sensor 7 = Extrnl Volt  9  surface irradiance (SPAR), degrees = 0.0
# datcnv_date = Jan 30 2011 03:29:38, 7.18
# datcnv_in = C:\SeaBirdDataProcessing\185_OISO19\st9\la26_1900_oiso19_09d.dat C:\SeaBirdDataProcessing\185_OISO19\precalib2010_noNMEA_TCPTC.CON
# datcnv_skipover = 0
# wildedit_date = Jan 30 2011 03:30:36, 7.18
# wildedit_in = C:\SeaBirdDataProcessing\185_OISO19\st9\la26_1900_oiso19_09d.cnv
# wildedit_pass1_nstd = 2.0
# wildedit_pass2_nstd = 20.0
# wildedit_pass2_mindelta = 0.000e+000
# wildedit_npoint = 100
# wildedit_vars = prDM depSM t090C c0S/m sal00 potemp090C sigma-é00 v0 sbeox0Mm/Kg v2 flECO-AFL flECO-AFL dz/dtM
# wildedit_excl_bad_scans = yes
# filter_date = Jan 30 2011 03:31:05, 7.18
# filter_in = C:\SeaBirdDataProcessing\185_OISO19\st9\la26_1900_oiso19_09d.cnv
# filter_low_pass_tc_A = 0.030
# filter_low_pass_tc_B = 0.150
# filter_low_pass_A_vars = depSM sal00 potemp090C sigma-é00 v0 sbeox0Mm/Kg v2 flECO-AFL flECO-AFL dz/dtM
# filter_low_pass_B_vars = prDM
# loopedit_date = Jan 30 2011 03:31:55, 7.18
# loopedit_in = C:\SeaBirdDataProcessing\185_OISO19\st9\la26_1900_oiso19_09d.cnv
# loopedit_percentMeanSpeed: minV = 0.250, ws = 300, percent = 20.00                                                      
# loopedit_surfaceSoak: do not remove                                                                                     
# loopedit_excl_bad_scans = yes
# Derive_date = Jan 30 2011 03:32:46, 7.18
# Derive_in = C:\SeaBirdDataProcessing\185_OISO19\st9\la26_1900_oiso19_09d.cnv C:\SeaBirdDataProcessing\185_OISO19\precalib2010_noNMEA_TCPTC.CON
# derive_time_window_dzdt = seconds: 2
# binavg_date = Jan 30 2011 03:33:22, 7.18
# binavg_in = C:\SeaBirdDataProcessing\185_OISO19\st9\la26_1900_oiso19_09d.cnv
# binavg_bintype = decibars
# binavg_binsize = 1
# binavg_excl_bad_scans = yes
# binavg_skipover = 0
# binavg_surface_bin = no, min = 0.000, max = 0.000, value = 0.000
# file_type = ascii
*END*
