* Sea-Bird SBE 9 Data File:
* FileName = C:\SBE_DATA\185_OISO19\La21_0542_Oiso19_O5D.hdr
* Software Version Seasave V 7.20g
* Temperature SN = 1821
* Conductivity SN = 2317
* Number of Bytes Per Scan = 37
* Number of Voltage Words = 5
* Number of Scans Averaged by the Deck Unit = 1
* Append System Time to Every Scan
* System UpLoad Time = Jan 21 2011 05:41:27
** Ship: MD FNIN
** Station: 05 D
** Latitude:  42 29.96 S
** Longitude: 052 29.05 E
** Operator: bo
** descente
# nquan = 18
# nvalues = 1000                        
# units = specified
# name 0 = nbf: Bottles Fired
# name 1 = prDM: Pressure, Digiquartz [db]
# name 2 = depSM: Depth [salt water, m]
# name 3 = t090C: Temperature [ITS-90, deg C]
# name 4 = c0S/m: Conductivity [S/m]
# name 5 = sal00: Salinity, Practical [PSU]
# name 6 = potemp090C: Potential Temperature [ITS-90, deg C]
# name 7 = sigma-é00: Density [sigma-theta, Kg/m^3]
# name 8 = dz/dtM: Descent Rate [m/s]
# name 9 = scan: Scan Count
# name 10 = sbeox0Mm/Kg: Oxygen, SBE 43 [umol/Kg]
# name 11 = depSM: Depth [salt water, m], lat = 40
# name 12 = sal00: Salinity, Practical [PSU]
# name 13 = potemp090C: Potential Temperature [ITS-90, deg C]
# name 14 = sigma-é00: Density [sigma-theta, Kg/m^3]
# name 15 = dz/dtM: Descent Rate [m/s], WS = 2
# name 16 = nbin: number of scans per bin
# name 17 = flag: flag
# span 0 =          0,          0       
# span 1 =      4.000,   1002.000       
# span 2 =      3.948,    991.931       
# span 3 =     2.7893,    12.1677       
# span 4 =   3.140656,   3.891589       
# span 5 =    33.7534,    34.4438       
# span 6 =     2.7231,    12.1670       
# span 7 =    25.6177,    27.4658       
# span 8 =     -0.837,      1.614       
# span 9 =         61,      29429       
# span 10 =    180.463,    308.591      
# span 11 =      3.970,    991.929      
# span 12 =    33.7534,    34.4438      
# span 13 =     2.7231,    12.1670      
# span 14 =    25.6177,    27.4659      
# span 15 =     -0.536,      1.622      
# span 16 =          6,        124      
# span 17 = 0.0000e+00, 0.0000e+00      
# interval = decibars: 1                
# start_time = Jan 21 2011 05:41:27
# bad_flag = -9.990e-29
# <Sensors count="15" >
#   <sensor Channel="1" >
#     <!-- Frequency 0, Temperature -->
#     <TemperatureSensor SensorID="55" >
#       <SerialNumber>1821</SerialNumber>
#       <CalibrationDate>19-Nov-10 </CalibrationDate>
#       <UseG_J>1</UseG_J>
#       <A>0.00000000e+000</A>
#       <B>0.00000000e+000</B>
#       <C>0.00000000e+000</C>
#       <D>0.00000000e+000</D>
#       <F0_Old>0.000</F0_Old>
#       <G>4.87571262e-003</G>
#       <H>6.89355063e-004</H>
#       <I>3.03221299e-005</I>
#       <J>2.60451786e-006</J>
#       <F0>1000.000</F0>
#       <Slope>1.00000000</Slope>
#       <Offset>0.0000</Offset>
#     </TemperatureSensor>
#   </sensor>
#   <sensor Channel="2" >
#     <!-- Frequency 1, Conductivity -->
#     <ConductivitySensor SensorID="3" >
#       <SerialNumber>2317</SerialNumber>
#       <CalibrationDate>19-Nov-10 </CalibrationDate>
#       <UseG_J>1</UseG_J>
#       <!-- Cell const and series R are applicable only for wide range sensors. -->
#       <SeriesR>0.0000</SeriesR>
#       <CellConst>2000.0000</CellConst>
#       <ConductivityType>0</ConductivityType>
#       <Coefficients equation="0" >
#         <A>0.00000000e+000</A>
#         <B>0.00000000e+000</B>
#         <C>0.00000000e+000</C>
#         <D>0.00000000e+000</D>
#         <M>0.0</M>
#         <CPcor>-9.57000000e-008</CPcor>
#       </Coefficients>
#       <Coefficients equation="1" >
#         <G>-1.07859966e+001</G>
#         <H>1.47329303e+000</H>
#         <I>-1.75348756e-004</I>
#         <J>7.37392413e-005</J>
#         <CPcor>-9.57000000e-008</CPcor>
#         <CTcor>3.2500e-006</CTcor>
#         <!-- WBOTC not applicable unless ConductivityType = 1. -->
#         <WBOTC>0.00000000e+000</WBOTC>
#       </Coefficients>
#       <Slope>1.00000000</Slope>
#       <Offset>0.00000</Offset>
#     </ConductivitySensor>
#   </sensor>
#   <sensor Channel="3" >
#     <!-- Frequency 2, Pressure, Digiquartz with TC -->
#     <PressureSensor SensorID="45" >
#       <SerialNumber></SerialNumber>
#       <CalibrationDate>02-May-2005</CalibrationDate>
#       <C1>-4.471217e+004</C1>
#       <C2>7.207370e-002</C2>
#       <C3>1.279440e-002</C3>
#       <D1>3.850500e-002</D1>
#       <D2>0.000000e+000</D2>
#       <T1>2.993439e+001</T1>
#       <T2>-2.595180e-004</T2>
#       <T3>3.740980e-006</T3>
#       <T4>3.368070e-009</T4>
#       <Slope>0.99995000</Slope>
#       <Offset>-0.39210</Offset>
#       <T5>0.000000e+000</T5>
#       <AD590M>1.118000e-002</AD590M>
#       <AD590B>-8.461320e+000</AD590B>
#     </PressureSensor>
#   </sensor>
#   <sensor Channel="4" >
#     <!-- Frequency 3, Free -->
#   </sensor>
#   <sensor Channel="5" >
#     <!-- Frequency 4, Free -->
#   </sensor>
#   <sensor Channel="6" >
#     <!-- A/D voltage 0, Oxygen, SBE 43 -->
#     <OxygenSensor SensorID="38" >
#       <SerialNumber>0563</SerialNumber>
#       <CalibrationDate>21-Dec-2010</CalibrationDate>
#       <Use2007Equation>1</Use2007Equation>
#       <CalibrationCoefficients equation="0" >
#         <!-- Coefficients for Owens-Millard equation. -->
#         <Boc>0.0000</Boc>
#         <Soc>0.0000e+000</Soc>
#         <offset>0.0000</offset>
#         <Pcor>0.00e+000</Pcor>
#         <Tcor>0.0000</Tcor>
#         <Tau>0.0</Tau>
#       </CalibrationCoefficients>
#       <CalibrationCoefficients equation="1" >
#         <!-- Coefficients for Sea-Bird equation - SBE calibration in 2007 and later. -->
#         <Soc>4.9690e-001</Soc>
#         <offset>-0.4999</offset>
#         <A>-1.4575e-003</A>
#         <B>-8.3681e-006</B>
#         <C> 2.8411e-007</C>
#         <D0> 2.5826e+000</D0>
#         <D1> 1.92630e-004</D1>
#         <D2>-4.64800e-002</D2>
#         <E> 3.6000e-002</E>
#         <Tau20> 1.2600</Tau20>
#         <H1>-3.3000e-002</H1>
#         <H2> 5.0000e+003</H2>
#         <H3> 1.4500e+003</H3>
#       </CalibrationCoefficients>
#     </OxygenSensor>
#   </sensor>
#   <sensor Channel="7" >
#     <!-- A/D voltage 1, Free -->
#   </sensor>
#   <sensor Channel="8" >
#     <!-- A/D voltage 2, Fluorometer, WET Labs ECO-AFL/FL -->
#     <FluoroWetlabECO_AFL_FL_Sensor SensorID="20" >
#       <SerialNumber>FLRTD-102</SerialNumber>
#       <CalibrationDate>15-Dec-2003</CalibrationDate>
#       <ScaleFactor>6.44400000e+000</ScaleFactor>
#       <Vblank>0.0920</Vblank>
#     </FluoroWetlabECO_AFL_FL_Sensor>
#   </sensor>
#   <sensor Channel="9" >
#     <!-- A/D voltage 3, Free -->
#   </sensor>
#   <sensor Channel="10" >
#     <!-- A/D voltage 4, Free -->
#   </sensor>
#   <sensor Channel="11" >
#     <!-- A/D voltage 5, Free -->
#   </sensor>
#   <sensor Channel="12" >
#     <!-- A/D voltage 6, Free -->
#   </sensor>
#   <sensor Channel="13" >
#     <!-- A/D voltage 7, Free -->
#   </sensor>
#   <sensor Channel="14" >
#     <!-- SPAR voltage, Unavailable -->
#   </sensor>
#   <sensor Channel="15" >
#     <!-- SPAR voltage, SPAR/Surface Irradiance -->
#     <SPAR_Sensor SensorID="51" >
#       <SerialNumber></SerialNumber>
#       <CalibrationDate></CalibrationDate>
#       <ConversionFactor>0.00000000</ConversionFactor>
#       <RatioMultiplier>0.00000000</RatioMultiplier>
#     </SPAR_Sensor>
#   </sensor>
# </Sensors>
# datcnv_date = Jan 25 2011 07:08:04, 7.20g
# datcnv_in = C:\SeaBirdDataProcessing\185_OISO19\st5\la21_0542_oiso19_o5d.hex C:\SeaBirdDataProcessing\185_OISO19\st5\la21_0542_oiso19_o5d.XMLCON
# datcnv_skipover = 0
# datcnv_ox_hysteresis_correction = yes
# datcnv_ox_tau_correction = yes
# wildedit_date = Jan 25 2011 07:09:48, 7.20g
# wildedit_in = C:\SeaBirdDataProcessing\185_OISO19\st5\la21_0542_oiso19_o5d.cnv
# wildedit_pass1_nstd = 2.0
# wildedit_pass2_nstd = 20.0
# wildedit_pass2_mindelta = 0.000e+000
# wildedit_npoint = 100
# wildedit_vars = prDM depSM t090C c0S/m sal00 potemp090C sigma-é00 dz/dtM sbeox0Mm/Kg
# wildedit_excl_bad_scans = yes
# filter_date = Jan 25 2011 07:09:56, 7.20g
# filter_in = C:\SeaBirdDataProcessing\185_OISO19\st5\la21_0542_oiso19_o5d.cnv
# filter_low_pass_tc_A = 0.030
# filter_low_pass_tc_B = 0.150
# filter_low_pass_A_vars = depSM sal00 potemp090C sigma-é00 dz/dtM sbeox0Mm/Kg
# filter_low_pass_B_vars = prDM
# loopedit_date = Jan 25 2011 07:10:15, 7.20g
# loopedit_in = C:\SeaBirdDataProcessing\185_OISO19\st5\la21_0542_oiso19_o5d.cnv
# loopedit_percentMeanSpeed: minV = 0.250, ws = 300, percent = 20.00                                                      
# loopedit_surfaceSoak: do not remove                                                                                     
# loopedit_excl_bad_scans = yes
# Derive_date = Jan 25 2011 07:10:28, 7.20g
# Derive_in = C:\SeaBirdDataProcessing\185_OISO19\st5\la21_0542_oiso19_o5d.cnv C:\SeaBirdDataProcessing\185_OISO19\st5\LA21_0542_OISO19_O5D.XMLCON
# derive_time_window_dzdt = seconds: 2
# binavg_date = Jan 25 2011 07:10:41, 7.20g
# binavg_in = C:\SeaBirdDataProcessing\185_OISO19\st5\la21_0542_oiso19_o5d.cnv
# binavg_bintype = decibars
# binavg_binsize = 1
# binavg_excl_bad_scans = yes
# binavg_skipover = 0
# binavg_surface_bin = no, min = 0.000, max = 0.000, value = 0.000
# file_type = ascii
*END*
